Delhi Metro, Phase III,





lots CC-18 and CC-23

an existing motorway bridge and addition of a new bridge

|  |  |
| --- | --- |
| General Data: | |
| **Project:** | Delhi Metro extension |
| **Client:** | **FEMC-Pratibha JV** |
| **Delivery period:** | 2013 - 2014 |
| **Scope of work:** | Extension of the Delhi Metro, CC-18 belongs to line 7 (ring line), CC-23 belongs to line 8 (outer ring line)   * 2 TBM-driven tunnels, length 16,4 km, external diameter 6,35 m, 11715 rings of 5+1 segments |
| Sealing method: | Maximum hydraulic pressure 3 bars  Test pressure 6 bars at worst combination of 4 mm gap and 15 mm offset  TunnelFlex 33 coex, Rubber gaskets with 90° Soft corners |
|  | TS 33x10 (7) coex E 209 |
| **Additional information:** | ES Rubber Ltd. | Kibbutz Ein Shemer | M.P. Hefer 38816, Israel | +972.4.637.1037 | [export@esrubber.com](mailto:export@esrubber.com) | www.esrubber.com  Dr. Werner Grabe mobile +49 174 6884223 |